                          Upload Information Template for Hobbes.nmsu.edu
                          ===============================================

        Archive Filename: nasm-3.01.zip
       Short Description: nasm v3.01 for OS/2
        Long Description: nasm v3.01 for OS/2.
nasm - the Netwide Assembler, a portable 80x86 assembler.

v3.01:
    * Added `obj2' output format for OS/2
        - Default attributes for a segment are ALIGN=16 and USE32.
        - Add a segment to FLAT group implicitly if 32-bit segment.
        - Recognize Unix sections .text, .rodata, .data and .bss as TEXT32,
          CONST32, DATA32 and BSS32 respectively for compatibility with other
          Unix platforms.
        - Set default classes implicitly for known segments such as TEXT32,
          CONST32, DATA32, BSS32 and so on.

    * Changed `GROUP' directive to be cumulative
    * Improved misc.


      Proposed directory
           for placement:  /pub/os2/dev/proglang/asm

               Your name: KO Myung-Hun
           Email address: komh78@gmail.com
    Program contact name: (same)
   Program contact email: (same)
             Program URL: * offical: https://github.com/netwide-assembler/nasm
                          * OS/2 port: https://github.com/komh/nasm-os2

      Would you like the
   contact email address
    included in listings? no

Operating System/Version: 
 Additional requirements: LIBCn v0.1.13(rpm)
                          * For build: gcc v15.2.0

                Replaces: (none)
