COPYRIGHT INTELLIGRAPHICS, INC. 1995

This is release B7 of the P9710 OS/2 PM display driver.  For
installation instructions please see INSTALL.TXT.

Restrictions in this release:

- Problems with host blt I/O (mono expand) require a software
  workaround.

- Starting VDMs in the background does not work correctly because
  the 9710 BIOS uses the extended registers to set the video mode,
  and VVIDEO does not trap them.

- VDMs have problems in all 640x480 resolutions due to the BIOS
  not setting bits 5-6 of index 5 of the GCPC register (3ce/3cf)
  correctly.

- There is an apparent problem in the vector drawing engine, in which
  the last pixel drawn is sometimes the wrong color.

EnDIVE:
  - When a movie is overlapped by a window the movie window goes blank.
    This is a bug in EnDIVE.

  - When a window is moved over a movie the "drag" border is in the
    background.  This is an EnDIVE bug.

  - Software cursors are not displayed when over a movie.

  - When the movie window is minimized the movie image is still displayed.
    This is an EnDIVE bug.


